<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40" y2="0" width="0" layer="20"/>
<wire x1="40" y1="0" x2="40" y2="40" width="0" layer="20"/>
<wire x1="40" y1="40" x2="0" y2="40" width="0" layer="20"/>
<wire x1="0" y1="40" x2="0" y2="0" width="0" layer="20"/>
<text>Receiver 003</text>
<text>OPENCORE NMR</text>
<text>2015 June K.T</text>
<text>+5</text>
<text>G</text>
<text>SIG IN</text>
<text>REF IN</text>
<text>IF OUT</text>
<hole x="2.5" y="2.5" drill="3.5"/>
<hole x="37.5" y="2.5" drill="3.5"/>
<hole x="37.5" y="37.5" drill="3.5"/>
<hole x="2.5" y="37.5" drill="3.5"/>
<text>G</text>
<text>2.5V</text>
<text>RFC</text>
<text>A0</text>
<text>A1</text>
<text>G/V</text>
<text>RF1</text>
<text>RF2</text>
<text>RF3</text>
<text>RF4</text>
<text>U3</text>
<text>JP1</text>
<text>JP2</text>
<text>JP3</text>
</plain>
<libraries>
<library name="miniCircuits">
<packages>
<package name="AT224">
</package>
</packages>
</library>
<library name="HIROSE">
<packages>
<package name="U.FL-R-SMT">
</package>
<package name="DF13-2P-12.5V">
</package>
<package name="DF13-3P-1.25V">
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="1608">
</package>
<package name="1005">
</package>
</packages>
</library>
<library name="ferriteBead">
<packages>
<package name="1608">
<description>1608-sized chip element
   by K. Takeda  2007.6.10</description>
</package>
</packages>
</library>
<library name="capacitor">
<packages>
<package name="3216_POLAR">
</package>
<package name="1608">
<description>1608-sized chip element
   by K. Takeda  2007.6.10</description>
</package>
<package name="1005">
<description>1005-sized chip element
         by K. Takeda 2007.6.10</description>
</package>
</packages>
</library>
<library name="AnalogDevices">
<packages>
<package name="AD8343">
</package>
</packages>
</library>
<library name="connector">
<packages>
<package name="SMA_STRAIGHT">
</package>
</packages>
</library>
<library name="nmr">
<packages>
<package name="MC74VHC1G04">
</package>
<package name="ADG904_TSSOP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor" package="3216_POLAR" value="10u">
<attribute name="NAME"/>
</element>
<element name="C8" library="capacitor" package="1608" value="0.01u">
<attribute name="NAME"/>
</element>
<element name="CN3" library="HIROSE" package="U.FL-R-SMT" value="">
<attribute name="NAME"/>
</element>
<element name="T1" library="miniCircuits" package="AT224" value="TC4-1W+">
<attribute name="NAME"/>
</element>
<element name="U1" library="AnalogDevices" package="AD8343" value="AD8343">
<attribute name="NAME"/>
</element>
<element name="T3" library="miniCircuits" package="AT224" value="TC4-1W+">
<attribute name="NAME"/>
</element>
<element name="T2" library="miniCircuits" package="AT224" value="TC1-1-13M+">
<attribute name="NAME"/>
</element>
<element name="CN2" library="HIROSE" package="U.FL-R-SMT" value="">
<attribute name="NAME"/>
</element>
<element name="FB2" library="ferriteBead" package="1608" value="FERRITEBEAD">
<attribute name="NAME"/>
</element>
<element name="R1" library="resistor" package="1608" value="510">
<attribute name="NAME"/>
</element>
<element name="C3" library="capacitor" package="1005" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C4" library="capacitor" package="1005" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C6" library="capacitor" package="1005" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C7" library="capacitor" package="1005" value="0.01u">
<attribute name="NAME"/>
</element>
<element name="R2" library="resistor" package="1608" value="68">
<attribute name="NAME"/>
</element>
<element name="R4" library="resistor" package="1005" value="10">
<attribute name="NAME"/>
</element>
<element name="R5" library="resistor" package="1005" value="10">
<attribute name="NAME"/>
</element>
<element name="R6" library="resistor" package="1005" value="10">
<attribute name="NAME"/>
</element>
<element name="R7" library="resistor" package="1005" value="10">
<attribute name="NAME"/>
</element>
<element name="R3" library="resistor" package="1608" value="68">
<attribute name="NAME"/>
</element>
<element name="CN1" library="connector" package="SMA_STRAIGHT" value="SMASTRAIGHT">
<attribute name="NAME"/>
</element>
<element name="CN5" library="HIROSE" package="DF13-2P-12.5V" value="">
<attribute name="NAME"/>
</element>
<element name="U2" library="nmr" package="MC74VHC1G04" value="MC74VHC1G04">
<attribute name="NAME"/>
</element>
<element name="CN4" library="HIROSE" package="DF13-2P-12.5V" value="DF13-2P-1.25V">
<attribute name="NAME"/>
</element>
<element name="U3" library="nmr" package="ADG904_TSSOP" value="ADG904"/>
<element name="CN8" library="HIROSE" package="U.FL-R-SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN9" library="HIROSE" package="U.FL-R-SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN10" library="HIROSE" package="U.FL-R-SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN11" library="HIROSE" package="U.FL-R-SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN12" library="HIROSE" package="U.FL-R-SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN7" library="HIROSE" package="DF13-2P-12.5V" value="DF13-2P-1.25V">
<attribute name="NAME"/>
</element>
<element name="CN6" library="HIROSE" package="DF13-3P-1.25V" value="">
<attribute name="NAME"/>
</element>
<element name="C2" library="capacitor" package="1005" value="0.01u">
<attribute name="NAME"/>
</element>
<element name="R8" library="resistor" package="1608" value="100">
<attribute name="NAME"/>
</element>
<element name="C5" library="capacitor" package="1005" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C9" library="capacitor" package="3216_POLAR" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+5V">
<contactref element="C1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="FB2" pad="2"/>
<contactref element="U1" pad="P$5"/>
<contactref element="C7" pad="1"/>
<contactref element="CN5" pad="2"/>
<contactref element="U2" pad="P$5"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="C1" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="CN3" pad="P$3"/>
<contactref element="CN3" pad="P$2"/>
<contactref element="CN2" pad="P$2"/>
<contactref element="CN2" pad="P$3"/>
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$14"/>
<contactref element="U1" pad="P$11"/>
<contactref element="U1" pad="P$8"/>
<contactref element="U1" pad="P$7"/>
<contactref element="C6" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="T1" pad="3"/>
<contactref element="CN1" pad="2"/>
<contactref element="CN1" pad="5"/>
<contactref element="CN1" pad="3"/>
<contactref element="CN1" pad="4"/>
<contactref element="T3" pad="4"/>
<contactref element="CN5" pad="1"/>
<contactref element="T2" pad="6"/>
<contactref element="C7" pad="2"/>
<contactref element="U2" pad="P$3"/>
<contactref element="CN4" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="T1" pad="1"/>
<contactref element="CN1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="T3" pad="2"/>
<contactref element="FB2" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="T3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="P$13"/>
</signal>
<signal name="N$22">
<contactref element="T3" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="P$12"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="P$9"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="P$10"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="C4" pad="2"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="C3" pad="2"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="P$4"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="P$2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="P$3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="T1" pad="6"/>
</signal>
<signal name="N$34">
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="T1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="CN3" pad="P$1"/>
<contactref element="T3" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="CN2" pad="P$1"/>
<contactref element="T2" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="P$6"/>
<contactref element="U2" pad="P$4"/>
</signal>
<signal name="N$1">
<contactref element="CN4" pad="1"/>
<contactref element="U2" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="CN12" pad="P$1"/>
<contactref element="U3" pad="P$10"/>
</signal>
<signal name="N$3">
<contactref element="CN10" pad="P$1"/>
<contactref element="U3" pad="P$7"/>
</signal>
<signal name="N$4">
<contactref element="CN8" pad="P$1"/>
<contactref element="U3" pad="P$4"/>
</signal>
<signal name="N$5">
<contactref element="CN9" pad="P$1"/>
<contactref element="U3" pad="P$17"/>
</signal>
<signal name="N$6">
<contactref element="CN11" pad="P$1"/>
<contactref element="U3" pad="P$14"/>
</signal>
<signal name="3.3V">
<contactref element="CN7" pad="2"/>
<contactref element="U3" pad="P$2"/>
<contactref element="R8" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="CN6" pad="2"/>
<contactref element="U3" pad="P$20"/>
</signal>
<signal name="N$12">
<contactref element="CN6" pad="1"/>
<contactref element="U3" pad="P$19"/>
</signal>
<signal name="GND2">
<contactref element="U3" pad="P$11"/>
<contactref element="U3" pad="P$12"/>
<contactref element="U3" pad="P$13"/>
<contactref element="U3" pad="P$15"/>
<contactref element="U3" pad="P$16"/>
<contactref element="U3" pad="P$18"/>
<contactref element="U3" pad="P$9"/>
<contactref element="U3" pad="P$1"/>
<contactref element="U3" pad="P$3"/>
<contactref element="U3" pad="P$5"/>
<contactref element="U3" pad="P$6"/>
<contactref element="U3" pad="P$8"/>
<contactref element="CN7" pad="1"/>
<contactref element="CN9" pad="P$2"/>
<contactref element="CN9" pad="P$3"/>
<contactref element="CN8" pad="P$3"/>
<contactref element="CN8" pad="P$2"/>
<contactref element="CN10" pad="P$3"/>
<contactref element="CN10" pad="P$2"/>
<contactref element="CN12" pad="P$3"/>
<contactref element="CN12" pad="P$2"/>
<contactref element="CN11" pad="P$2"/>
<contactref element="CN11" pad="P$3"/>
<contactref element="C5" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N2">
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="CN6" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
